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Refrigerated Circulators (XT5718LT Series)
For use in Laboratory or Industry 
 A reliable temperature control for process, environmental, 
microbiological and hazardous waste applications.
Patented stepper valve hot gas by-passing and dynamic temperature control for stability up to ± 0.1 °C, for continuous reliable operation 

Available with cooling capacity for 400 W, 800 W, 1,200 W, 1,600 W and 2,000 W 

Magnetic driven pump for quiet but powerful circulating, seamless liquid delivery and precise temperature control 
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Optional stepper valve driving, external Pt100 and RS232/485 interface for connection to a refrigerating condensing unit, external circulating application system for continuous reliable operation
Replacement for Julabo F250 & FL300 series , LAUDA Microcooler & WK, Huber Minichiller/ Unichiller, .Yamato CF and CLS series and PolyScience MM/LM/LS series 

Specifications:

	Models
	  XT5718LT-E1200-R40   
	  XT5718LT-E2000-R40 

	Temperature range@20℃
	-40～+40
	-40～+40

	Temperature stability±℃
	0.2～0.5
	0.2～0.5

	Cooling capacity@20℃W
	1200
	2000

	Pump pressure maxbar
	1.4
	1.4

	Pump flow-rate maxL/min
	25
	25

	Filling volume L
	5~10
	5～10

	Overall size mm
	460W×600D×825H
	500W×780D×1000H

	Protection against run-dry & spillage
	LLCO
	LLCO


	Models
	XT5718LT-E3000-R40
	XT5718LT-E5000-R40

	Temperature range@20℃
	-40～+40
	-40～+40

	Temperature stability±℃
	0.2～0.5
	0.2～0.5

	Cooling capacity@20℃W
	3000
	5000

	Pump pressure maxbar
	1.4
	1.4

	Pump flow-rate maxL/min
	25
	25

	Filling volume L
	5～10
	5～10

	Overall size mm
	600W×980D×1200H
	600W×1180D×1200H

	Protection against run-dry & spillage
	LLCO
	LLCO
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